### NZ FIRE DOORS - FIRE-RATED INTERIOR WINDOWS

 Window Reference ~

 Manufacturer: **NZ Fire Doors**

 Window type: I- 60 -TW

 Wall type: ~

 FRR: ~

 STC: ~

 Size: ~mm high x ~mm wide

 Frame thickness: 45mm

 Frame material: Hardwood

 Finish: Paint or other specified

 Glass type: ~

 Wall type: Concrete, Concrete Masonry, Timber frame, Steel frame, etc, (state linings)

 FRR: -/60/30, -/60/60 (Integrity & Insulation)

 STC: Varies. Contact NZ Fire Doors to confirm

 Size: Maximum glass area applies. Refer to Glazing clause

 Glass type: Schott Pyranova 15mm - FR up to -/60/30 minutes Integrity and Insulation

 Schott Pyranova 23mm - FR up to -/60/60 minutes Integrity and Insulation