### NZ FIRE DOORS - FIRE-RATED INTERIOR WINDOWS

Window Reference ~

Manufacturer: **NZ Fire Doors**

Window type: I- 60 -TW

Wall type: ~

FRR: ~

STC: ~

Size: ~mm high x ~mm wide

Frame thickness: 45mm

Frame material: Hardwood

Finish: Paint or other specified

Glass type: ~

Wall type: Concrete, Concrete Masonry, Timber frame, Steel frame, etc, (state linings)

FRR: -/60/30, -/60/60 (Integrity & Insulation)

STC: Varies. Contact NZ Fire Doors to confirm

Size: Maximum glass area applies. Refer to Glazing clause

Glass type: Schott Pyranova 15mm - FR up to -/60/30 minutes Integrity and Insulation

Schott Pyranova 23mm - FR up to -/60/60 minutes Integrity and Insulation