**Specification for Residential Windows & Doors**

1 July 2013

***ALTHERM RESIDENTIAL SUITE***

**2.1 AWNING and CASEMENT WINDOWS**

Windows shall be constructed using Altherm brand Residential frames, utilising a 35mm platform and an IGU thickness upto 22mm.

* Opening sashes include a cover facing and have both bead-glazed and pocket glazed options.
* Mullions and transoms have external fins for added strength where required.
* Include passive ventilation in the form of either;
  + Truvent – fitted to the head of the window, or
  + Vented Sash – fitted to the sill of an opening sash.

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*