**Specification for Residential Windows & Doors**

1 July 2013

***ALTHERM RESIDENTIAL SUITE***

**2.2 VERTICAL SLIDING WINDOWS**

*Two vertical sliding window options are available, the aluminium framed Double Hung window and the frameless Shugg window.*

**Double Hung Window**

Windows shall be constructed using the Altherm Double Hung Window frame, utilising either single glazing upto 6mm or double glazing upto 20mm.

* Frame options include either the Contemporary facing (01374) or Colonial facing (01373).

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*