**Specification for Residential Windows & Doors**

1 July 2013

***ALTHERM RESIDENTIAL SUITE***

**2.6 HINGED and FRENCH DOORS**

*Residential hinged and french doors are rated to 2.1m high in ‘very high’ wind zones.*

*For french doors rebated meeting stiles give a flush appearance and provide superior weathering. Parliament hinges allow doors to open a full 180° in a brick veneer application. A bottom rail extender is available to create a deep look in the classic french door style*

Doors shall be constructed using Altherm hinged door frames, utilising panels with an IGU thickness upto 22mm.

* Standard configuration

Open In / Open Out

Applies to Door No’s... *(or refer to the window schedule drawing)*

* Hardware as nominated in the hardware section.
* Options = ...

*(options = parliament hinges, bottom rail extender)*

Applies to Door No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*