**Specification for Smartwood Series Windows & Doors**

1 July 2013

***SMARTWOOD SERIES***

**7.1 AWNING and CASEMENT WINDOWS**

Windows shall be constructed using Smartwood Series frames utilising a 38mm platform and an IGU thickness up to 24mm (a special bead allows 32mm double glazed units with internal blind systems).

* Facing sashes are used.
* All windows are externally beaded.
* Sightline adaptors are available for continuous sightlines.
* Mullions and transoms project internally as solid wood profiles.
* Timber Species = ...
* Options = ...

*(options = sightline adaptors)*

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*