**Specification for Smartwood Series Windows & Doors**

1 July 2013

***SMARTWOOD SERIES***

**7.3 BI-FOLD WINDOWS**

Windows shall be constructed using the Smartwood Series bi-fold window frame and an IGU thickness up to 24mm.

* All profiles are from the Smartwood Series bi-fold door system with a smaller bottom rail.
* The window rolling gear slides on an externally projecting track.
* All windows are externally beaded.
* Timber Species = ...

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*