**Specification for Smartwood Series Windows & Doors**

1 July 2013

***SMARTWOOD SERIES***

**7.8 SLIDING DOORS**

*Smartwood sliding doors are rated to 2.2m high in ‘very high’ wind zones. They slide on an external track with fixed sidelight.*

Doors shall be constructed using the Smartwood Series sliding door frame and an IGU thickness up to 24mm.

* Overlights are possible.
* Sightline adaptors are available for continuous sightlines.
* All doors are externally beaded.
* Timber Species = ...
* Options = ...

*(options = sightline adaptors)*

Applies to Door No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*