**Specification for Smartwood Series Windows & Doors**

1 July 2013

***SMARTWOOD SERIES***

**7.2 HORIZONTAL SLIDING WINDOWS**

Windows shall be constructed using the Smartwood Series sliding window frame and an IGU thickness up to 24mm.

* Sliding windows slide on an external track and use the sliding door frame and a smaller bottom rail.
* Sightline adaptors are available for continuous sightlines.
* All windows are externally beaded.
* Timber Species = ...
* Options = ...

*(options = sightline adaptors)*

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*