**Specification for APL Architectural Series Windows & Doors**

1 July 2013

***ALTHERM - APL ARCHITECTURAL SERIES***

**6.8 SLIDING DOORS**

*APL Architectural Series sliding doors are rated to 2.7m high in ‘very high’ wind zones. They slide on an external track with either a fixed side panel or as a bypass configuration. Flush sill or rebated sill options are available. Stiffening boxes on interlocker stiles and mullions are flush in the closed position.*

Doors shall be constructed using the APL Architectural Series sliding door frame and an IGU thickness up to 26mm.

* Overlights are possible through the use of a coupling bar at the head of the Metro door frame.
* All doors are internally beaded using square edge beads.
* Corner sliders, bypass sliders, cavity sliders and over-wall sliders are available options, as indicated in the drawings / window schedule.

Applies to Door No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*