**Specification for Metro Series Thermal Heart Windows & Doors**

1 July 2013

***ALTHERM – METRO SERIES THERMAL HEART***

**5.2 HORIZONTAL SLIDING WINDOWS**

Windows shall be constructed using Metro Series Thermal Heart sliding window frames and an IGU thickness up to 24mm.

* The perimeter frame is the Metro Series Thermal Heart sliding door frame with smaller profiles for rails, stiles and mullions.
* Stiffening boxes on interlocker stiles and mullions align in the closed position.
* All windows are externally beaded with square edge rather than sloped beads.

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*