**Specification for Residential Series ThermalHEART Windows & Doors**

9 February 2023

***ALTHERM RESIDENTIAL SERIES THERMALHEART RANGE***

**3.1 AWNING and CASEMENT WINDOWS**

Windows shall be constructed using Residential Series ThermalHEART frames, utilising a 44mm platform with thermal break and an IGU thickness up to 24mm.

* Opening sashes are cover facing as standard.
* All windows are externally beaded with square edge beads.
* Mullions and transoms have external or internal stiffening fins depending on window span and wind load.

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*