***ALTHERM - APL ARCHITECTURAL SERIES THERMAL HEART*®**

**5.8 SLIDING DOORS**

*APL Architectural Series ThermalHEART***®** *sliding doors are rated to 3.0m high in ‘extra high’ wind zones. They slide on an external track with a fixed sidelight. Stiffening boxes on interlocker stiles and mullions align in the closed position.*

Doors shall be constructed using the Metro Series ThermalHEART**®** sliding door frame and an IGU thickness up to 44mm.

* Opening sashes are possible if placed away from the travel path of an opening door panel.
* Sidelights and overlights are possible through the use of either an integral mullion/transom or by coupling frames together with the Architectural coupling system.

Applies to Door No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*