**Specification for APL Architectural Series Windows & Doors**

1 July 2013

***FIRST – APL ARCHITECTURAL SERIES***

**6.1 AWNING and CASEMENT WINDOWS**

Windows shall be constructed using APL Architectural Series frames, and an IGU thickness up to 26mm.

* Two frame widths are offered – 106mm and 158mm, depending on the frame width of adjoining doors.
* Opening sashes are non-facing, fitting flush with the frame.
* All windows are externally beaded with square edge rather than sloped beads.

*( for single glazing there is an option to use sloping beads)*

* Mullions and transoms have internal box stiffeners.

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*