**Specification for APL Architectural Series Windows & Doors**

1 July 2013

***FIRST – APL ARCHITECTURAL SERIES***

**6.2 HORIZONTAL SLIDING WINDOWS**

Windows shall be constructed using APL Architectural Series sliding window frames and an IGU thickness up to 26mm.

* Sliding windows use the APL Architectural Series sliding door profiles.
* Stiffening boxes on interlocker stiles and mullions are flush in the closed position.
* Sliding windows are internally beaded using square edge beads.

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*