**Specification for Residential Windows & Doors**

1 July 2013

***FIRST RESIDENTIAL SUITE***

**2.3 BI-FOLD WINDOWS**

*This robust bi-fold system includes panels with square-cut corners and an in-frame track for direct window support. A wide range of open out configurations are available including the ‘lay-back’ option for 2-panel formats, which allows the panels to open back against an adjacent wall.*

Windows shall be constructed using FIRST bi-fold window frames, utilising an IGU thickness upto 22mm.

* Standard configuration

Applies to Window No’s... *(or refer to the window schedule drawing)*

* Lay-back configuration

*(only two panels per side can ‘lay-back’)*

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*