**Specification for Residential Windows & Doors**

1 July 2013

***FIRST RESIDENTIAL SUITE***

**2.2 HORIZONTAL SLIDING WINDOWS**

*Two horizontal sliding window options are available, the Slimline, which can only be single glazed, and the Slidemaster, which is a higher specification slider suitable for double glazing. The Slidemaster includes a ‘flushline’ sill and easy-glide panels for clean appearance and smooth operation.*

**Slidemaster Sliding Window**

Windows shall be constructed using the Slidemaster Sliding Window frame, utilising a 35mm platform and an IGU thickness upto 22mm.

* Panel lead stile options include either plain face (02721) or extruded finger pull (02730).
* Interlocker mullions options include either flat face (02886) or external box for larger spans (02723).
* Include passive ventilation in the form of;
	+ Truvent – fitted to the head of the fixed portion of the window.

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*