**Specification for Residential Thermal Heart Windows & Doors**

1 July 2013

***FIRST RESIDENTIAL THERMAL HEART RANGE***

**3.1 AWNING and CASEMENT WINDOWS**

Windows shall be constructed using Residential Thermal Heart frames, utilising a 46mm platform with thermal break and an IGU thickness up to 24mm.

* Opening sashes are cover facing as standard.
* All windows are externally beaded with choice of square edge or sloped beads.
* Mullions and transoms have external stiffening fins depending on window span and wind load.

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*