**Specification for Smartwood Series Windows & Doors**

1 July 2013

***SMARTWOOD SERIES***

**7.7 BI-FOLD DOORS**

*This bi-fold system is rated to 2.1m high in ‘very high’ wind zones. For a deep bottom rail bottom rail extenders can be used. A wide range of configurations are available.*

Doors shall be constructed using Smartwood bi-fold door frames, utilising panels with an IGU thickness up to 24mm.

* Standard configuration

Open Out

* Timber Species = ...
* Options = ...

*(options = bottom rail extender)*

Applies to Door No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*