
# K-MODA

The K-Moda updates the classic style partition system with modern design features. K-Moda features stainless steel blade mounted pedestals and updated hardware. The K-Moda system is available in the widest range of materials meaning more colour selection and the ability to choose from 13mm, 18mm or 33mm width front panels. It achieves all of this with the same quality and affordability of previous system designs.



## Laminate to choose from:

High Pressure Laminates Low Pressure Laminates Compact Laminates  
KerMac Decorative Melteca KerMac Compact  
Laminex Melamine Laminex Compact  
Formica Structural Board

## Applications Features

General Purpose Stainless Steel/Blade/Cast pedestal  
Wet or dry areas (Compact Only Wet Areas) Anodised Aluminium channels  
High Humidity (Compact only) Stainless Steel locks, coat hooks and fastenings



## Standard Materials

18mm thick MDF laminated board  
13mm Compact laminate  
18mm Structural Board  
Non-standard facing panels made to order  
For high humidity areas Interior Plywood available  
Anodised aluminium channel/headrail

Optional Accessories:  
Toilet roll holders  
Grab Rails  
Pull Handles  
Shower seats and brackets  
Paper towel dispenser  
Waste receptacles  
Powder coated aluminium trim

## Dimensions and installation

Width and depth vary to suit application  
Doors: Standard 600mm opening  
 Disabled 800mm minimum opening  
 Sliding doors on request  
Standard height is 2000mm with 200mm floor clearance  
  
KerMac include installation within the Auckland region. Alternatively, cubicles can be flat packed and shipped anywhere in Australasia with installation instructions included.

## CAD drawings

Larger CAD Drawings available on [www.kermac.co.nz](http://www.kermac.co.nz) in PDF, DWG and DXF formats

PH: (09) 273 1524 | ADDRESS: Unit I, 9 Lady Ruby Drive, East Tamaki, Auckland | PO Box 51

PH: (09) 273 1524 | ADDRESS: Unit I, 9 Lady Ruby Drive, East Tamaki, Auckland | PO Box 51 964