# K-proform

The K-Proform system is our high end design. It is finished in Post-formed edges that give it that sleek styled look. Blade type pedestals raise it off the floor.


## Laminate to choose from:

High Pressure Laminates
Wilsonart
Laminex
Formica
Nevamar

## Applications Features

Low moisture/dry area Box Blade pedestal
High end offices Anodised Aluminium channels
Commercial Stainless Steel locks, coat hooks and fastenings
Banks Rise and fall hinges
Museums



## Standard Materials

18mm/30mm thick MDF laminated board
Non-standard facing panels made to order
Edge-banded laminated board/Postformed edges

Optional Accessories:
Toilet roll holders
Grab Rails
Pull Handles
Shower seats and brackets
Paper towel dispenser
Waste receptacles
Powder coated aluminium trim

## Dimensions and installation

Width and depth vary to suit application
Doors: Standard 560mm opening
 Disabled 760mm minimum opening
 Sliding doors on request
Standard height is 1900mm with 100mm floor clearance

KerMac include installation within the Auckland region. Alternatively, cubicles can be flat packed and shipped anywhere in Australasia with installation instructions included.

## CAD drawings

Larger CAD Drawings available on [www.kermac.co.nz](http://www.kermac.co.nz) in PDF, DWG and DXF formats

PH: (09) 273 1524 | ADDRESS: Unit I, 9 Lady Ruby Drive, East Tamaki, Auckland | PO Box 51 964 Pakuranga, Auckland