IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2017-12-14T15:27:45"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20140709_2115(x64) - Exporter 2014.0.2014.0709 - Default UI"
Application: "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)"

People and organizations
  Person "dcole" of Organization (no name given)
  Owner history of Person "dcole" of Organization (no name given) | application "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)" | change NOCHANGE | created 1513265018 (2017-12-14T15:23:38Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  POWERUNIT: WATT

Spatial structure
IFCPROJECT | long name "P:\Fastrack\53721_DOLPHIN SOLUTIONS LIMITED\ADDITIONAL DRAWINGS 2017 BIM\IFC\DRYER UPDATES\BC2002.ifc"
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 2 elements
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Wall 1" | object type "Basic Wall:Wall 1:1494" | names: "Basic Wall:Wall 1:3092" | material: layers "Basic Wall:Wall 1" ("Default Wall" 50.) | property sets: Constraints, Phasing, Dimensions, Structural, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | object type "BC2002 Dolphin Eco Hand Dryer" | names: "BC2002:BC2002 Dolphin Eco Hand Dryer:60561" | material: materials ("Nozzle", "Stainless Steel") | property sets: Constraints, Dimensions, Phasing, Pset_ManufacturerTypeInformation, Pset_BuildingElementProxyCommon, Identity Data

Types
  IFCWALLTYPE "Basic Wall:Wall 1" | STANDARD | 1 occurrence | material: layers "Basic Wall:Wall 1" ("Default Wall" 50.) | property sets: Construction, Analytical Properties, Identity Data, Graphics

Property sets
  Constraints | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Finish Face: Interior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 936.966674301787 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 357.139423611487 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Phasing | properties | on 2 objects (1 IFCBUILDINGELEMENTPROXY, 1 IFCWALLSTANDARDCASE)
    Phase Created = "New Construction" (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 0.599658671553143 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 640. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0299829335776572 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Volume = 0.00699080357400224 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Height = "230mm" (IFCTEXT)
    Height above counter = "The unit should be minimum 300mm above the surface below." (IFCTEXT)
    Projection = "145mm" (IFCTEXT)
    Width = "246mm" (IFCTEXT)
  Structural | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Wall 1" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "Dolphin Solutions Limited" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "BC2002 Dolphin Eco Hand Dryer" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDING)
    Building Name = "" (IFCTEXT)
    NBSSpecificationPath = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Address = "Southpoint, Compass Park, Junction Road, Bodiam, TN32 5BS" (IFCTEXT)
    Assembly Code = "E1090900" (IFCTEXT)
    Assembly Description = "Other Equipment" (IFCTEXT)
    Description = "Eco hand dryer" (IFCTEXT)
    Email = "info@dolphinsolutions.co.uk" (IFCTEXT)
    Fax No. = "+44 (0) 1424 205200" (IFCTEXT)
    Manufacturer = "Dolphin Solutions Limited" (IFCTEXT)
    Model = "BC2002" (IFCTEXT)
    OmniClass Number = "23.80.30.11.17" (IFCTEXT)
    OmniClass Title = "Distribution Boards and Control Panels" (IFCTEXT)
    Tel No. = "+44 (0) 1424 202224" (IFCTEXT)
    URL = "www.dolphinsolutions.co.uk" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IPXI rated = TRUE (IFCBOOLEAN)
    SKA Rating Compliant = TRUE (IFCBOOLEAN)
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Product Data = "Very low operating power saving 80% or more of user's energy costs. Infra red self adjusting sensor. Heater on/off switch and adjustable airflow giving the potential for even greater energy savings. Dries hands in only 10-12 seconds with heater and full speed - reducing CO2 emissions drastically. Outlet temperature 55ºC (131ºF) at 25ºC (77ºF) ambient temperature with heater on and dryer at full speed. 3 year limited warranty. IPXI rated. Class 1 rated isolation. Average Reuse Rate under WEEE Directive: 78%. Average Recovery Rate under WEEE Directive: 956%. Ska compliant product. Unit should be mounted to give no less than 300mm clearance from the bottom of the unit to the nearest surface below." (IFCTEXT)
    Product Page Link = "https://www.dolphinsolutions.co.uk/product/eco-hand-dryer/" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "-3000010" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Graphics | properties | on 1 type object
    Coarse Scale Fill Color = 8454143 (IFCINTEGER)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Roughness = 1 (IFCINTEGER)