### NZ FIRE DOORS - FIRE-RATED INTERIOR WINDOWS

 Window Reference ~

 Manufacturer: **NZ Fire Doors**

 Window type: I- 30 -TW

 Wall type: ~

 FRR: -/30/30

 STC: ~

 Size: ~mm high x ~mm wide

 Frame thickness: 45mm

 Frame material: 45mm Pine

 Finish: Paint

 Glass type: Schott Pyranova 15mm

 Wall type: Concrete, Concrete Masonry, Timber frame, Steel frame, etc, (state linings)

 STC: Varies. Contact NZ Fire Doors to confirm

 Size: Maximum glass area applies. Refer to Glazing clause