### NZ FIRE DOORS - FIRE-RATED INTERIOR WINDOWS

Window Reference ~

Manufacturer: **NZ Fire Doors**

Window type: I- 30 -TW

Wall type: ~

FRR: -/30/30

STC: ~

Size: ~mm high x ~mm wide

Frame thickness: 45mm

Frame material: 45mm Pine

Finish: Paint

Glass type: Schott Pyranova 15mm

Wall type: Concrete, Concrete Masonry, Timber frame, Steel frame, etc, (state linings)

STC: Varies. Contact NZ Fire Doors to confirm

Size: Maximum glass area applies. Refer to Glazing clause