**Specification for Residential Windows & Doors**

1 July 2013

***ALTHERM RESIDENTIAL SUITE***

**2.4 LOUVRES**

*The Altair louvre system from Breezway, Australia, is factory fitted within most types of window or door frame. Glass, aluminium or timber louvre blades can be used in 102mm (4-inch) or 152mm (6-inch) widths. Breezway also offer a Stronghold system which offers increased security.*

* Type = Altair

*(type = Altair or Stronghold)*

* Colour matched to window frames...
* Blade type ...
* Blade depth ...

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*