**Specification for Residential Windows & Doors**

1 July 2013

***ALTHERM RESIDENTIAL SUITE***

**2.5 ENTRANCE DOORS**

*A selection of entrance door panel styles is offered;*

**Plasma Entrance Door**

*The Plasma delivers a solid, flat faced appearance that can be clad in a variety of materials, typically aluminium sheet or colour coated glass . Glazing infills can be cut into the panel if desired.*

* Type = ...
* Outer skin = ...
* Colour = ...
* Inner skin = 2mm aluminium sheet
* Colour = ...
* Glass option = ...
* Hardware as nominated in the hardware section

*(- type = eg 5906000*

 *- Outer & inner skins – either 2mm aluminium sheet or 5mm glass*

 *- glass options = eg cathedral, sandblasted, leadlight*

*Refer to your window fabricator for configuration / glass options)*

*For alternative options contact APL Technical Support*