**Specification for Residential Windows & Doors**

1 July 2013

***ALTHERM RESIDENTIAL SUITE***

**2.2 VERTICAL SLIDING WINDOWS**

*Two vertical sliding window options are available, the aluminium framed Double Hung window and the frameless Shugg window.*

**Shugg Window**

*The Shugg window system from Neotech, is factory fitted within most types of window or door frame. The units are typically double hung and single glazed, but other options are available. When single glazed there are no horizontal members. When double glazed the sashes utilise the Altherm Double Hung panel.*

* Type = Double Hung
* Colour matched to window frames...
* Glazing = Single
* Glass type ... *(refer to the Glass Options section)*

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*